# A ONE INTERIOR DESIGNER

BEST DESIGNS \* BEST QUALITY \*BEST PRICE

To

Dear Sir

Quotation for interior work .

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| S no |  | Description | Area | Unit | Rate/sq ft | Amount |
| 1. | a. | Kitchen  Base unit  Size:8.6’+3.3’\*2.6’=30.94 | 30.94 | sq ft | 1450 | 44,863 |
|  | b. | wall unit  Size:8.6’\*2’=17.2 | 17.2 | sq ft | 1150 | 19,780 |
|  | c. | loft fixed frame with doors  size:8.6+6.2’\*2.6’=38.48 | 38.48 | sq ft | 750 | 28,860 |
|  | d. | Accessories hettich/ebco  tandem boxs-3nos  IN & OUT Basket -3nos  PVC try-1nos  dustbin -1nos  G profile handles –6length  soft close hinges -10set  soft close channels –3set | 3  3  1  1  6  10  3 | no’s  no’s  no’s  no’s  length  set  set | 4750  3950  2250  1750  2350  480  850 | 14,250  11,850  2,250  1,750  14,100  4,800  2,550 |
|  | e. | utility storage base + middles  size:3.4’\*2.8’=9.52  size:3.7’\*2’=7.4  soft close hinges –5set | 9.52  7.4  5 | sq ft  sq ft  set | 1450  1150  480 | 13,804  8,510  2,400 |
|  |  | **kitchen total amount** | **103.54** |  |  | **169,767** |
| 2. | a. | MBR  wardrobe with dressing unit  size:7’\*8.9’=62.3  soft close hinges -9.5set  soft close channels -2set | 62.3  9.5  2 | Sq ft  set  set | 1250  480  850 | 77,875  4,560  1,700 |
|  | b. | loft fixed frame with doors  size:12’\*2.5’=30 | 30 | sq ft | 750 | 22,500 |
|  |  | **MBR total amount** | **101.8** |  |  | **106,635** |
| 3. | a. | KBR  Wardrobe swing open with puja unit  size:7’\*11’=77  soft close hinges -14set  soft close channels -3set | 77  14  3 | sq ft  set  set | 1250  480  850 | 96,250  6,720  2,550 |
|  | b. | study + books storage box  size:3.5’\*2.6’=9.1  size:3.5’\*2’=7  soft close hinges -2set | 9.1  7  2 | sq ft  sq ft  set | 950  1150  480 | 8,645  8,050  960 |
|  | c. | loft fixed frame with doors  size:11’\*2.5’=27.5 | 27.5 | sq ft | 750 | 20,625 |
|  |  | **KBR total amount** | **120.6** |  |  | **143,800** |
| 5. | a. | Hall  crockery unit  size:7’\*2’=14  soft close hinges =4set  soft close channels -1set | 14  4  1 | sq ft  set  set | 1150  480  850 | 16,100  1,920  850 |
|  | b. | Breakfast counter + panelling  size:3’\*3=9  size:5’\*1’=5  size:6’\*1’=6 | 9  5  6 | sq ft  sq ft  sq ft | 950  750  750 | 8,550  3,750  4,500 |
|  | c. | TV unit  size:1’\*7.3’=5.6  size:7’\*1.7’=11.9  size:5’\*1.7’=8.5  size:5’\*5.6=28  soft close hinges -2set  soft close channels -4set | 5.6  11.9  8.5  28  2  4 | sq ft  sq ft  sq ft  sq ft  set  set | 1150  1150  1150  750  480  850 | 6,440  13,685  9,775  21,000  960  3,400 |
|  | d. | Washbasin + mirror + loft  size:3’\*3’=9  size:3’\*2.5’=7.5  soft close hinges -2set | 9  7.5  2 | sq ft  sq ft  set | 1450  750  480 | 13,050  5,625  980 |
|  | e. | Shoe rack with sitting  size:3’\*1.5’=4.5  size:3’\*1.9’=5.7  soft close hinges -3set  soft close channels -1set | 4.5  5.7  3  2 | sq ft  sq ft  set  set | 1150  1150  480  850 | 5,175  6,555  1,440  1,700 |
|  |  | **Hall total amount** | **114.7** |  |  | **125,455** |
|  |  | **Total amount**  **Add: Transport+ shifting**  **Net Total amount**  **Net total amount** | **440.64** |  |  | **545,657**  **8,000**  **553,657**  **550,000** |
|  | a.  b.  c.  d. | Additional work  fall ceiling Based on designs  Electrical work wiring + lights  tiles & Granite work  2D & 3D designs |  |  |  |  |

**Payment terms and conditions:**

**1.** Booking advance 5% (finalise designs and laminate)

2. Advance payment 45 % (structure)

3. Second stage 30% (doors fixing).

4. Third stage 10% (handles and glass).

5. after completion of project 10%. (After complete everything)

**Material details:**

1. 19mm club prime 710 grades BWP kitchen bottom cabinet remaining area 18mm century saink ply wood doors 19mm block board back side 6mm ply with laminate sheet.

2. Inside.8mm half white laminate outside give regular sf finish. Kitchen only hi glossy . Remaining area matt finish. Hi glossy 1500 to 2500 rupees per sheet extra.

3. All drawers’ channels hettich normal inside. Drawers lock hettich or godraj Europa.

4. All door hinges hettich soft close. Lofts normal .

5. All hettich tandem boxes. Stainless steel IN & OUT baskets .

6. Termite proof ply wood only we have using.

7. Factory work done pasting, cutting, edge bending and doors.

8. Flat do assembly some outside laminate pasting and hard ware fittings.

9. Two year free service all fittings.

10. Handles 4”=150, 6”=180, 8” -200, and 10”-220.

Samraj @Shyam

Client signature Authorized signature